#!/bin/sh
CARD=$(pactl list cards short | grep '1f.3' | awk '{print $2}')
CURRENT_SINK=$(pactl info | grep "Default Sink:")
dunstctl close-all
case $CURRENT_SINK in
  *iec958*)
    pactl set-card-profile $CARD output:analog-stereo
    notify-send "analog out active" -i :
    ;;
  *)
    pactl set-card-profile $CARD output:iec958-stereo
    notify-send "digital out active" -i :
    ;;
esac
